# IBM LAN Support Program:
installing the NDIS2 driver

The Madge NDIS2 driver for DOS is called MCBND.DOS. To install it, follow the instructions below:

1. Run the IBM DXMAID utility. When asked if you are using driver diskettes answer Yes.
2. In the Process Driver Diskette box, type the path A:\DOS.
3. Continue through the installation process choosing the protocols and interfaces you need, and changing any parameters you need to change.
4. When you have finished, reboot the computer.