Banyan Vines 6.0 Server                                      May 1997
=======================                                      ========

CAUTION
=======

The LSS.500\vines directory contains a  pre-release  version  of  the
image for Banyan Vines 6.0 servers.  It  has  NOT  been as thoroughly
tested as the main LSS 5.0(2) drivers.


How to Install the Banyan Vines Driver 
======================================

1)  Create a Driver Diskette
    ------------------------
    From a DOS workstation, use Madge Wizard  to  create  an  install
    disk.  To do this put an  unformatted  disk  in drive A:\ and run
    MWIZARD.EXE from either the hard disk or the CD-ROM drive. Select
    the following options :
            - Read Documentation
            - Install disks (from the toolbar)
            - LSS 5.0(0)
            - VINES.BWR from list 
            - Run script
    This will create a Banyan Vines driver image on drive A:\.

2)  To Install the Driver
    ---------------------
    Follow the instructions below.
      (1)  From  the  Service Monitor, select "4-Exit".
      (2)  From  the  Operator menu, select "10-System Maintenance".
      (3)  From  the  System  Maintenance   menu,  select   "6-Server 
           Configuration".
      (4)  Select "8-Install Remove Drivers".
      (5)  Insert the driver disk, created above,  in to  drive  A:\.
           Press enter to load driver.
      (6)  Confirm driver name and press enter.
      (7)  Remove disk once copying of files is complete.
      (8)  Press enter (twice), as directed by the on screen prompts.
      (9)  Select "Save configuration and exit".

    The driver should now be installed.
      (10) From  the  Server  Configuration  menu,  select  "1 - Add
           cards ..." .
      (11) Select "Add".
      (12) Choose  the appropriate Madge adapter from the list.  For
           this pre-release driver the name of the card is  prefixed
           with "NEW".
      (13) Configure card parameters as required.
      (14) Select "Save & Exit".
      (15) Return to the Operator menu.
      (16) Select 4 to shutdown the server.

After shutdown, re-boot the server and confirm that the Madge driver
loads reporting the following version numbers :-
     NIC Driver Ver 1.0.00, SLDK Ver 2.0.00
      