# Configuring Your Ringnode to use the Smartrom

| Before inserting the Ringnode, switch off the power to your computer. Power off your computer, before inserting or removing any option boards.

| If you want to protect the configuration of your Ringnode, set a password.

For configuration information, select your Ringnode:

AT Plus Ringnode, PCI (BM) 2 Ringnode, or ISA Client Plus Ringnode

AT Ringnode, ISA Client Ringnode, Fiber AT Ringnode, or PC Ringnode

MC Ringnode or MC32 Ringnode

EISA Ringnode