Dedicated Token Ring Drivers
============================
                                                             May 1997
                                                             -------- 

This file provides an overview of  the  environments  under which the 
Dedicated Token Ring (DTR) drivers have been verified.

CAUTION
=======

The DTR drivers in this section can be substituted for the equivalent 
drivers in the main  LSS 5.0  release.   However,  they have not been 
tested  under the  same range  of conditions  as the LSS 5.0 drivers. 
They  are  pre-release  drivers.  You  are  advised  to evaluate them 
carefully before  using them  in  new  environments.   These  drivers
have  the  same  names  as  the  LSS  5.0  drivers,  but  they   have 
different major version numbers. Inclusion of drivers in this section
does  not  imply that  features  within  these  drivers  will  become
standard in future releases.


DTR Server Drivers
==================
Server drivers have been  provided  for  use  in  the  IBM LanServer, 
Netware and Windows NT environments.


IBM LanServer
-------------
In the \lss.500\dtr\lansrv\os2 directory you will find an  OS/2 NDIS2
driver.
This driver has NOT been updated in LSS 5.0(2).

Novell Netware
--------------
In the \lss.500\dtr\netware\server directory you will find a  Netware
4.x server driver.

This driver has been updated in LSS 5.0(2) and hence contains  all of
the fixes that the LSS 5.0(1) driver contains.  It  also  contains an
additional  fix  to  reduce CPU  utilization in Netware 4.10 servers. 


Windows NT
----------
In the \lss.500\dtr\winnt\i386  directory  you  will find a  miniport
driver. 

This driver  has  NOT  been  updated  in  LSS 5.0(2).

