# Madge Blue+ 16/4 ISA PnP adapter

The highest performing fully IBM-compatible Token Ring ISA adapter.

- Overview
- Description
- Specifications
- Ordering Information

## Overview

The Blue+ 16/4 ISA PnP Adapter provides the unparalleled combination of faster overall network performance with guaranteed interoperability with legacy IBM environments.

It is ideal for all ISA-based PCs that need to support both the latest operating systems and also access older host-based applications, which require full register-level IBM compatibility. Blue+ 16/4 ISA PnP has the flexibility to run either IBM's shared RAM Token Ring drivers or Madge's performance enhancing FastBlue software.

### Customer Benefits

- Simplified support and installation
- Guaranteed 100% IBM compatibility
- Risk-free upgrade for IBM desktops

### Key Features

- Ultimate performance for ISA PCs
- Runs IBM LSP 1.2+ AND Madge FastBlue software
- Up to 2 1/2 x the throughput of equivalent IBM adapters

## Description

- Introduction
- Unparalled performance
- Compatibility and versatility
- Flexibility
- Customer support

Combining ease of use with optimum performance for the latest desktop operating environments, the Blue+ 16/4 ISA PnP adapter has the versatility to support the Token Ring networking needs of today and tomorrow.

### Introduction

The Blue+ 16/4 ISA PnP adapter is the latest addition to Madge's extensive range of desktop networking solutions. It is uniquely suited to meet the rigorous computing demands of customers wishing to remain 100% IBM compatible throughout their network.

Blue+ 16/4 ISA PnP provides the unparalleled combination of faster network performance and 100% IBM compatibility by using Madge's RingRunner technology, which is fully compliant with the IEEE 802.5 Token Ring standard. It provides users with an easy upgrade for their installed adapters which no longer offer the levels of performance needed to run todays applications over Token Ring.

The Madge Blue+ 16/4 ISA PnP adapter and Fast Blue software provide the performance needed to unlock the power of todays advanced client software applications.

### Unparalled Performance

Business computing platforms are changing, driven by sophisticated network-oriented applications. It is therefore essential to use network adapters which offer the highest levels of performance to satisfy evolving business needs in todays client/server networks. With Plug and Play installation and automatic ring speed detection, the latest network adapters become an integral part of a client PC, easing administrative support overhead and reducing maintenance costs.

Every Blue+ 16/4 ISA PnP ships with Madges unique Fast Blue software, a set of enhanced network drivers for all popular network operating systems. Using Fast Blue drivers, the Blue+ 16/4 ISA PnP has been proven to deliver up to 2 1/2 times the performance of IBM shared memory adapters. Users can access distributed databases more quickly and achieve faster response times from intensive client/server applications.

### Compatibility & Versatility

The Blue+ 16/4 ISA PnP is a plug-compatible replacement for IBM adapters and seamlessly supports IBM drivers and applications. Customers desktop investment is protected since Blue+ 16/4 ISA PnP will work with past, present and future network applications designed for IBM environments. Re-training costs are minimised as system configuration and installation procedures are similar.

Fast Blue drivers are compatible with IBM's shared-memory adapters and enhance these adapters' performance by up to 25%, replacing* IBMs LAN Support Program . Upgrade existing IBM adapters with Fast Blue drivers and reap the benefits of maintaining a common driver set for IBM and Madge adapters - and increase network performance! Fast Blue software also offers memory savings for DOS users by loading drivers into extended/expanded memory, releasing conventional memory to support desktop applications.

### Flexibility Installation and configuration is simplified by the plug and play capabilities of Blue+ 16/4 ISA PnP, or by using Madge's Windows-style GUI in non-PnP situations. Once a standard configuration has been created, it can be quickly and simply copied network-wide to other PCs equipped with the Blue+ 16/4 ISA PnP. Soft configuration eliminates the need to open PCs to change switch settings, saving LAN technicians time.

Blue+ 16/4 ISA PnP has on-board ring speed detection and Madges Auto WireSense to automatically determine the speed and media type of the Token Ring connection. This gives users the ability to easily move PCs to different rings on a network, saving time and support overhead.

### Customer Support Without Limits

The Blue+ 16/4 ISA PnP is backed by Madge's world-renowned expertise in networking. Madge's worldwide service and support organization continues to satisfy the needs of our worldwide installed base in the most demanding Global 1000 companies.

A worldwide network of field service engineers provide a wide range of technical services including on-site technical support and software upgrades. Customers can also download up-to-date technical information from on-line services such as CompuServe or can contact the Madge World Wide web home page. (http://www.madge.com). The Madge Blue+ 16/4 ISA PnP comes with a lifetime** hardware warranty and a 30-day installation guarantee, which includes free technical hotline support and on-site assistance as required.

## Specifications

    Network type:               4 or 16 Mbps IBM and IEEE 802.5 Token Ring,
                                with optional Automatic Ring Speed Detect
    Supply voltage:             +5V DC 5%
    Power:                      3W Maximum
    Bus interface:              16-bit ISA compatible
                                Full Plug and Play support
    Bus transfer:               Shared Memory
    Ring interface:             RJ45 socket (UTP)
                                9-pin D-type socket (STP)
    EMC certification:          FCC Class A
                                EN55022 Class B (STP)
                                EN55022 Class A (UTP)
    Memory:                     256KB dynamic RAM on-board
    IRQ options:                2, 3, 6, 7, 10, 11, 12, 15
    I/O options:                0A20, 0A24
    Boot ROM:                   On-board RPL
    Software support:           IBM LSP v1.2+ -OR- Madge FastBlue software v2.1+
    Dimensions:                 167mm x 90mm
    Weight:                     0.11 Kg (approx)
    Temperature range:          0-50 degrees C
    Humidity range:             10% - 80% non-condensing
    Warranty period:            Lifetime**

* Subject to license

** Full details available upon request

## Ordering Information

Blue+ ISA 16/4 ISA Adapter (including Madge FastBlue user license)

    Part No         Description                 Qty
    62-04           Blue+ 16/4 ISA PnP           1
    62-14           Blue+ 16/4 ISA PnP          10
    62-24           Blue+ 16/4 ISA PnP          20
    62-34           Blue+ 16/4 ISA PnP          30
    62-54           Blue+ 16/4 ISA PnP          50

Fast Blue User License (For IBM adapters)

    Part No         Description                Qty
    84-16           User License                10
    84-17           User License                50
    84-18           User License               250