# Configuration information for the MC and MC32 Ringnodes

To configure the MC or MC32 Ringnode, copy the .ADF files from the Madge release disk onto the reference disk supplied with your computer. Then run the computer's configuration utility, and enable the Smartrom. The addresses in memory that the Smartrom image can be mapped to are:

C4000-C5FFF
C6000-C7FFF
CC000-CDFFF
CE000-CFFFF
D4000-D5FFF
D6000-D7FFF
DC000-DDFFF
DE000-DFFFF