# Installing the NDIS2 driver using LAPS

1. Insert the LAPS disk into the floppy drive.
2. Run LAPS.EXE.
3. Click Install.
4. Specify a target driver and click OK.
5. Click Exit.
6. Change to the IBMCOM folder by double-clicking on it in the Drive C window.
7. Run LAPS.EXE.
8. Click Install.
9. Put the Madge CSS Release Disk into the floppy drive, and type the path A:\OS2. Click OK.
10. Click Configure.
11. Check Configure LAN transports.
12. Click Continue.
13. In the Network Adapters box, select Madge 16/4 CardBus Adapter.
14. Click Add.
15. In the Protocols box, select the protocols you need, and click Add.
16. Click Exit.
17. Click Continue.
18. Click OK.
19. Click Exit.
20. Remove the floppy disk, then shut down and reboot the system.