# Installing the UnixWare 2.0 Driver

The driver supports following adapter cards:

Smart 16/4 AT Ringnode/Bridgenode
Smart 16/4 AT Plus Ringnode
Smart 16/4 ISA Client Ringnode
Smart 16/4 ISA Client Plus Ringnode
Smart 16/4 EISA Ringnode/Bridgenode
Smart 16/4 MC Ringnode/Bridgenode
Smart 16/4 MC32 Ringnode/Bridgenode

Before installing the driver, create an installation disk. To do this:

1. Log into your Unixware system as the system owner.

2. Copy the mdgunx2.img file from the Madge CD into the /tmp directory.

3. Place a blank formatted 3.5-inch disk in drive A: and enter the command:
   dd if=/tmp/mdgunx2.img of=/dev/fd0135ds18

   This creates a installable version of the driver on the floppy disk.

   ### To install the driver:

   1. Log onto your Unixware system as the system owner.

   2. From the Desktop menu, select the Admin_Tools icon.

   3. From the System Setup folder, select the Appl_Installer icon.

   4. From the Appl_Installer application, click on the Update View button.

   5. Select the madgeodi icon, and click on the Install button.

   6. When prompted by Unixware, answer the questions about the configuration of the Madge Token Ring adapters in your computer.

   7. When you have completed the installation reboot your computer.