# Installing the NDIS2 driver using MPTS

1. Put MPTS Disk 1 into the folppy drive.
2. Run MPTS.EXE.
3. At the Welcome screen, click OK.
4. Click Install.
5. Specify a target drive, and click OK.
6. Click Install.
7. Insert disks and click OK as prompted.
8. When the MPTS installation is complete, click OK.
9. Click Configure.
10. Click Configure again.
11. In the LAPS Configuration dialog, click Other Adapters...
12. Put the Madge CSS Release Disk into the floppy drive, and type A:\OS2.
13. Click OK.
14. From the list of network adapters, select Madge 16/4 CardBus Adapter.
15. Click Add.
16. From the protocols list, select the protocols you require, and click Add.
17. Click OK.
18. Click Close.
19. Click Exit.
20. Click Exit again.
21. Click OK.
22. Click Exit.
23. Remove the Madge CSS Release Disk from the floppy drive.
24. Shut down and reboot the PC.