# IBM DOS LAN Services

To install IBM DOS LAN Services on a workstation:

1. Insert the DOS LAN Services Disk 1 into the floppy drive. Type A:\
2. Type Install then press ENTER.
3. Follow the on-screen instructions. Confirm the adapter's settings. When asked to select a network driver, choose the No network adapter option.
4. Proceed with the installation, inserting disks when necessary.
5. Reboot the computer when the installation is complete.
6. Run the Install program from the directory that you installed DOS LAN Services into.
7. Select To install an additional network driver from disk.
8. Insert the Madge CSS Release Disk, and type the path: A:\DOS
9. Select the CardBus Adapter.
10. Complete the installation and then restart your computer.