### Index of Adapter Software TechNotes

    06101-04  SMARTIPX parameters

    06201-04  SMARTLSP parameters

    06401-01  Installing an NDIS driver for DOS workstations under Banyan VINES

    06602-03  Smart Software: configuring multiple Ringnodes

    06603-04  Smart Software: the SMTLINK combination utility

    06607-01  Smart Software: selecting interfaces

    06608-01  Smart Software: installing interfaces

    06609-01  Smart Software: host parameters

    06610-01  Smart Software: card parameters

    06611-01  Smart Software: LLC parameters

    06612-01  Smart Software: NetBIOS parameters

    06613-01  Smart Software: IPX parameters

    06614-01  Smart Software: ODI parameters

    06615-01  Smart Software: TCP/IP parameters

    06616-01  Smart Software: NOVAPI parameters

    06617-01  Smart Software: RARPD parameters

    06618-01  Smart Software: configuring for source-routing bridges

    06619-01  Smart Software: backwards compatibility

    06620-02  Smart Software: NDIS parameters

    06701-04  Installing NetWare using MADGEODI for DOS

    06801-07  Madge driver support for SCO UNIX workstations

    06802-02  Madge driver support for IBM RISC System/6000 AIX stations

    06803-02  Madge driver support for Solaris UNIX stations

    06804-02  Madge driver support for UnixWare stations

    06902-02  Supporting Microsoft Windows for Workgroups version 3.11

    07001-01  Installing the Madge Card Services software for DOS or OS/2

    07002-01  Installing the Madge PCMCIA Ringnode using Toshiba Cardware