# Configuring the Smart 16/4 MC Ringnode

The Smart 16/4 MC Ringnode is configured using the reference diskette which should be supplied with your computer. If you have configured option boards before, you will find this straightforward. The process consists of two steps: first, copy the @002D.ADF file from the Madge distribution diskette onto your reference diskette, and then run either:

- The automatic configuration option.

- The manual configuration option.

For further information about the configuration options refer to the @002D.ADF file which is in a readable form.