# Madge Token Ring Adapters

Madge provides the industry's broadest range of intelligent adapters for Token Ring networks. Madge adapters are designed to bring out the best in every networked desktop, irrespective of the PC platform, resident operating system, or applications running on users' desktops.

Compatible with all popular client and server operating systems and PC environments, Madge adapters are the ideal choice for companies seeking a single source Token Ring desktop solution from end-to-end. Easy t use menu-based software can create a standard set-ip for any networked PC and reduces the suppotr overhead and complexity of managing large number of desktops.

### Smart 16/4 Ringnodes

Madge Smart 16/4 Ringnodes provide the industry's broadest range of intelligent adapters for Token ing networks. These are supported by a common suite of LAN Support Software (LSS) network drivers and installation utilities that enable a standard network configuration script to be deployed network-wide, irrespective of the PC bus types used.

### Blue+ 16/4 Adapters

Madge Bue+ adapters provide the unrivaled combination of excellent performance for ISA bus PC's and 100% compatibility with IBM LAN Support Program. Madge FastBlue performance enhancing software allows customers to deploy a single high throughput driver implementation for both Madge Blue and IBM shared memory adapters, with no impact upon applications compatibility.

## Key Features:

- Supports all popular desktop & notebook PCs
- Fully compliant with IEEE 802.5 standards
- Interoperable with IBM Token Ring products
- Supported by common software suite
- Dedicated Token Ring ready
- Lifetime warranty

General purpose clients | High-end clients | Workgroup servers | Enterprise servers
Blue+ ISA | Blue+ ISA |  |
Blue+ PnP | Blue+ PnP |  |
Smart ISA PnP |  |  |
Smart AT Plus | Smart AT Plus | Smart AT Plus |
Smart AT PnP | Smart AT PnP | Smart AT PnP |
Smart PCI | Smart PCI | Smart PCI | Smart PCI
| Smart EISA | Smart EISA | Smart EISA
Smart MC | Smart MC |  |
|  | Smart MC32 | Smart MC32
Smart PCMCIA