# ATPMODE.EXE command-line options

The command-line options that you can use with ATPMODE.EXE.

Command-line | Description
/MODE= | can be normal (normal mode) or at (AT mode).
/IO= | is the hexadecimal IO address of the Ringnode you want to configure.
/LIST | Display the current software operating mode of the selected Ringnode in your workstation.
/SECURE | Prevent the Ringnode from using pre-LSS 4.3 software.
/? | Display help information.