# Windows for Workgroups:
installing the ODI driver

The Madge ODI driver for DOS is called MCBODI.COM. To install it, follow the instructions below:

1. Run the NetWare Client INSTALL program.
2. Select Other Drivers. When prompted for a disk, insert the Madge CSS Release Disk.
3. Type A:\DOS as the path of the driver software.
4. Select Madge 16/4 CardBus Adapter.
5. Continue through the program. When you have finished, shut down and reboot the PC.

- Installing Windows for Workgroups but connecting only to NetWare
- Installing Windows for Workgroups, connecting to NetWare, and connecting to a Windows for Workgroups network

### Installing Windows for Workgroups but connecting only to NetWare

1. Install NetWare 4.1 client software with support for Windows. This procedure involves installing all the necessary Windows files into the Windows directory.
2. Start Windows.
3. From the Main Group window, select Windows Setup, then from Options, select Network Settings....
4. From the Network setup dialog box, select Networks.
5. Select Install Windows support for the following network only.
6. Move down the options list. If you have NetWare 4.1 client installed, select Novell NetWare (Workstation Shell 4.0 and above). If you have NetWare 3.x client installed, select Novell NetWare (Workstation Shell 3.X).
7. The setup procedure asks for some support files. These files are on Novell's WINUP9 disk or the latest VLMUP kit. Both the WINUP9 disk and the latest VLMUP kit are available from the Novell Bulletin Board.

### Installing Windows for Workgroups, connecting to NetWare, and connecting to a Windows for Workgroups network

1. Install NetWare 4.1 client software with support for windows. The installation will install all relevant windows files into the Windows directory.
2. Start up Windows.
3. From the Main Group window, select Windows Setup, then from Options, select Network Settings....
4. From the Network setup dialog box, select Drivers.
5. Select Add Adapter. From the adapter list, select Unlisted Adapters.
6. Put the Madge CSS Release Disk into the floppy drive.
7. In the install driver box, type the path A:\DOS
8. Select the Madge 16/4 CardBus Adapter.
9. Select the ODI driver.
10. Click Close.
11. Click Continue.
12. Select Workgroup names and workstation names. The setup procedure then asks for relevant support files. These files are located on Novell's WINUP9 disk or latest VLMUP kit. You can find both of these on the Novell Bulletin Board.
13. Restart your computer.
14. Edit the PROTOCOL.INI file in the Windows directory. In the PROTOCOL.INI file, make sure bindings=MCBODI. If it doesn't, change all bindings= statements to bindings=MCBODI.