# Remote booting troubleshooting

If your PCMCIA Ringnode fails to initialize, ensure that you have specified the following in your MDGBOOT.CFG file:
card_services=yes

or that you select Madge Card Services at the menu when you run the remote boot loaded utility. If your Smart 16/4 ISA Client PnP Ringnode fails to initialize, ensure that you have specified the following in your REMBOOT.CFG file:
enable_pnp=yes

or that you enable the Plug 'n' Play software at the menu, when you run the remote boot loaded utility.