# Installing the MDGND.DOS (NDIS2) driver

To install MDGND.DOS:

1. Run the Windows NT SETUP program.

2. Select Other Drivers, from the Network Adapter Drivers box. When prompted, insert the Madge release disk.

3. Select All Madge Smart 16/4 Ringnodes (MDGND.DOS).

4. Select the protocols you require, and continue through the SETUP process.

5. Save the configuration and exit from SETUP.

6. Reboot your computer.