Madge Smartrom image files
==========================
                                               LSS 5.0(0), August 1996
                                               -----------------------

This  file explains the purpose of the different Madge Smartrom images 
supplied with this release.

For instructions on how to program these images into the Smartrom, see 
the SMARTROM.TXT file, and the User Documentation. 


MULTI.ROM  ........ Use  this image on software programmable Ringnodes 
                    such as the AT Plus and ISA Client Plus Ringnodes.  
                    It contains a Ringnode  configuration  utility,  a 
                    Remote  Reset module and an RPL module. The Remote 
                    Reset   and   RPL   modules   support   the   same 
                    environments  as  the  NW.ROM  and NRPL.ROM images 
                    described below.  For  more information,  see  the 
                    SMARTROM.TXT file.

NRPL.ROM   ........ Use this image for Ringnodes that are to boot from 
                    a Novell NetWare server running  the  RPL NLM,  or 
                    from an IBM LAN Server or a Microsoft  LAN Manager 
                    server.
                     
NW.ROM     ........ Use  this  image for Ringnodes that are to boot by
                    Remote Reset from a Novell NetWare server.
            

            ***** End of ROMIMAGE.TXT *****
