# Advanced Power Management

## Driver Support

Advanced power management is supported in the following LSS 5.0 drivers :

- ODI Client driver for DOS - MADGEODI.COM
- ODI Client driver for OS/2 - MADGEODI.SYS
- NDIS2 driver for DOS - MDGND.DOS
- NDIS2 driver for OS/2 - MDGND.OS2

Under Windows 95 and Windows NT, power management is a function of the operating system and not the individual driver. When a PC enters a power-saving mode, the operating system asks the driver to shut itself down, and when power is restored the system loads the driver again. Hence, there is no specific power management support in Madge drivers for these operating systems.

Note that Smart Software (SMART.EXE and .SMT modules) does not support power management.

### Enabling APM under MDGND.XXX

In order to enable the power management features for MDGND.DOS you must include the following line in the driver section of your PROTOCOL.INI :

         APM = YES

For the OS/2 driver (MDGND.OS2), power management is enabled by default. To disable this feature include the following line in the driver section your PROTOCOL.INI :

         APM = NO

### Enabling APM under MADGEODI.XXX

In order to enable the power management features of MADGEODI.COM you must include the following line in the driver section of your NET.CFG :

         LINK DRIVER MADGEODI
              Power Management

For the OS/2 driver (MADGEODI.SYS), power management is enabled by default.