# How to configure remote booting

### Introducing the Madge Smartrom

### Installing your Smartrom

### Enabling and configuring your Smartrom

### Configuring your Ringnode to use the Smartrom

### Setting up the server for remote booting

### Troubleshooting

| If your Ringnode does not have a Smartrom or you want to remote boot from a floppy disk, do so using the Remote Boot Loader utility, REMBOOT.EXE.