# Sample SMART.CFG files

Sample configuration of IPX, NDIS, and LLC

Figure 1 shows a sample file for enabling and configuring IPX, NDIS, and LLC on a Smart 16/4 Ringnode.

    [HOST]			; Host-specific parameters.
     win=31			; Set up for Windows 3.1
     load.high		; Run SMART.EXE in Upper Memory.

     [CARD]			; Ringnode-specific parameters.
     frame.size=4096	; Max framesize is 4096 bytes.

     [IPX]			; IPX interface enabled.
     source.routing=y	; IPX source routing enabled.

     [NDIS]			; NDIS interface enabled.
     max.transmits=15	; Queue up to 15 messages to send.
     max.indications=15	; Queue up to 15 received messages.

     [LLC]			; LLC interface enabled.
     pcs			; AS/400 support.
     rx.size=2000		; LLC receive frames limited to 2000
    			; bytes.
     stations=80		; 80 LLC links available to NetBIOS.
     extra.stations=10	; 10 extra links for other LLC applications

Figure 1 Sample SMART.CFG files for Smart IPX, NDIS and LLC

Sample configuration of TCP/IP

Figure 2 shows a sample file for enabling and configuring the Smart TCP/IP suite of protocols on a Smart 16/4 Ringnode.

    [HOST]		; Host-specific parameters.
    win=31			; Set up for Windows version 3.1.
    load.high		; Run SMART.EXE in Upper Memory.

    [CARD]			; Ringnode-specific parameters.

    [NOVAPI]		; LAN WorkPlace for DOS interface.
    enable.statistics=no	; Disable MIB information (saves
    			; 2kbytes of DOS memory).

    [TCP]			; TCP interface enabled.
    tcp.requests=32		; Allow the Ringnode to operate
    			; with a high number (32) of
    			; outstanding TCP commands.

    [IP]			; IP interface enabled.
    enable.mib=no		; Disable MIB (to improve
    			; performance).

    [UDP]			; UDP interface enabled.
    udp.ports=2		; Only two UDP ports required.

    [DHCP]
    dhcp.bootp=yes		; BOOTP support

Figure 2 Sample SMART.CFG file for Smart TCP/IP