# Using Madge ODI drivers to remote boot from NetWare servers

This section tells you how to set up a boot image suitable for remote booting from a NetWare server, using either the Remote Reset or RPL booting scheme. The Madge drivers you can use are MADGEODI.COM or Smart ODI.

### NetWare Remote Reset

For Remote Reset, run the Novell program RPLODI.COM before running the ODI driver. RPLODI preserves the network connection until you have run IPXODI.COM. Figure 1 shows a sample AUTOEXEC.BAT file.

>       REM Sample autoexec.bat file for use with Remote Reset.

>       lsl

>       REM run rplodi.com to preserve the network connection.
>       rplodi
>       REM now run the driver.

>       madgeodi
>       ipxodi
>       route

>       netx ps=thor

>       login thor

Figure 1. Sample AUTOEXEC.BAT file for NetWare Remote Reset

### NetWare RPL

For NetWare RPL, do not run RPLODI.COM: the Smartrom maintains the network connection itself until you have run IPXODI.COM.

>       REM Sample autoexec.bat file for use with NetWare RPL.
>       lsl
>       madgeodi
>       ipxodi
>       route
>       netx ps=thor
>       login thor

Figure 2. Sample AUTOEXEC.BAT file for NetWare RPL