# The command-line options for PNPENABL.EXE

Specify the following command-line options:

/IO= | is the hexadecimal I/O address of the Ringnode you want to configure.
/INT= | is the interrupt (IRQ) channel you want the Ringnode to use. Valid values are 2, 3, 5*, 7, 10, 11, and 15.

*on the latest versions of this Ringnode only

The following command-line parameters are optional:

/QUIET | Suppresses all screen output.
/NOMORE | Disables the screen paging facility.
/? | Displays help information.

For example: `PNPENABL /IO=0A20 /INT=10 /QUIET`

enables the ISA Client PnP Ringnode at I/O 0a20 and using an IRQ 10. The screen output is also suppressed.