# Using the Multi-Protocol Transport Services (MPTS) configuration program to install the Madge driver, MDGND.OS2

MPTS is supplied with the following products:

- IBM LAN Server
- IBM Extended Services for OS/2
- IBM Network Transport Services/2

You can also use it to configure protocols for:

- IBM Communications Manager/2
- IBM Database Manager/2

To install MDGND.OS2:

1. Run the Multi-Protocol Transport Services (MPTS) configuration program by clicking on the MPTS icon in the LAN Services File and Print folder.

2. Insert the Madge release disk into a floppy drive.

3. Click on Install.

4. Type the path of the directory A:\OS2 which is where the drivers are stored. MPTS copies the files from the Madge release disk.

5. Shutdown and reboot your computer.

6. Select Configure LAN transports from the Configuration box. In the Configure Workstation window:

   (If IBM Token-Ring Network Adapter appears in the Current Configuration box, remove the protocols for the adapter individually, and then remove the adapter name)

> i Add Madge Fastmac Plus OS/2 NDIS MAC driver for Smart 16/4 Ringnodes to the list in the Current Configuration box.

> ii Add all of the protocols you need to the list in the Current Configuration box. Basic operation for LAN Server Requesters requires IBM OS/2 NETBIOS. If you are using IBM host connectivity, select IBM IEEE 802.2 as well.

> iii To view or change parameters in PROTOCOL.INI, select Edit.

> iv Complete installation by following the on-screen instructions.

> v Shutdown and reboot the computer.