# Testing a Ringnode

1. The screen displays the Madge Smart Ringnode Diagnostics window. Highlight a Ringnode in the "Ringnodes and Bridgenodes Found" box.

2. Press [F4]

3. Testing begins. The screen displays test statistics in the top right corner and gives a short explanation of the current test.

   To get help: | Press [F1]
   To pause testing: | Press [F6]
   To resume testing: | Press [F6]