# Before configuring your Smartrom using SMARTROM.EXE

The Madge Smartrom is supplied with a Smartrom image already loaded. The Madge Smartrom images are:

- MULTI.ROM (for greater flexibility and for PCI Ringnodes).

- NW.ROM (for NetWare Remote Reset).

- NRPL.ROM (for Remote Program Load).

Before running the Smartrom configuration software:

- Install the Smartrom (unless you have an AT Plus, PCI Fiber, or EISA Fiber Ringnode).

- Install and configure the Ringnode, enabling the Smartrom.

- Run the diagnostics program (unless you have diskless workstations).

| If you have any memory management software in your workstation, ensure that it does not remap the area of upper memory required by the Smartrom. For example with DOS, use the X= parameter on the EMM386 command line, or the RAM= parameter on the 386MAX command line. The addresses used by the Smartrom are given in the Ringnode configuration section.