# Sample SMART.CFG

    ;---------------------------------------------------------------------------;

    [host]
    ; DISPLAY                   ;    Displays protocols being loaded
    ; FORCELOAD                 ;    Overloads existing software running
    ; WIN=31                    ;    Windows Compatability
    ; HIGH                      ;    Loads software high
    ; PC3270=101                ;    PC3270 Compatabilty Set correct version

    [CARD]                      ;    This Section loads Parameters to card
    ; PIO                       ;    Avoids DMA problems with memory managers
    ; LOMEM                     ;    Avoids DMA problems with Programmed I/O Trans.
    ; FRAME.SIZE=4096           ;    Specifies Frame size for IPX and NetBios
    ; NODE.ADDRESS=400012345678 ;    Sets the Locally Administerd Address
    ; SAPS=10                   ;    This is for LLC Service Access Points
    ; EXTRA.STATIONS=20         ;    This is for Extra Stations
    ; EXTRA.SAPS=5              ;    This is for Extra Saps

    [IPX]                       ;    This section is for IPX
     SR=Y                       ;    This is for Source Routing
     CO=25                      ;    This is for Connections Default is 3

    ;[NOVAPI]                   ;    This is the host's Interface

    ;[IP]                       ;    This is for IP addressing
    ; IP.ADDRESS=193.35.4.21    ;    This is for Host's IP Address
    ; IP.ROUTER=193.35.4.99     ;    This is for network's Router

    ;[UDP]                      ;    Please view Info File for more Parms

    ;[TCP]                      ;    Please View info file for more Parms

    ;[NETB]                     ;    This Section is for Netbios
    ; TX.U.BUFFERS=25           ;    This is for Internal Buffer handling
    ; S=24                      ;    This is for Netbios Sessions Default is 4
    ; C=24                      ;    This is for Netbios Commands Default is 10

    ;[LLC]                      ;    This Section is for IEEE 802.2
    ; RX.SIZE=2130              ;    Default is frame size is 2130
    ; PCS                       ;    For PC Support product

    ;[ODI]                      ;    This section is for ODI
    ; FRAME TOKEN-RING          ;    Frames for IPX/SPX
    ; FRAME TOKEN-RING_SNAP     ;    Frames for IP Frames
    ; ODI.NSUP=YES              ;    Use with Novells ODINSUP

    ;[CARD]                     ;    This Section is for a Second card
    ; PIO                       ;    Avoids DMA problems with memory managers
    ; IO=1a20                   ;    Specifies I/O Location

    ;[NETB]                     ;    This Section is for Netbios
    ; TX.U.BUFFERS=25           ;    This is for Internal Buffer handling
    ; S=24                      ;    This is for Netbios Sessions Default is 4
    ; C=24                      ;    This is for Netbios Commands Default is 10

    ;[IPX]                      ;    This section is for IPX
    ; SR=Y                      ;    This is for Source Routing
    ; CO=25                     ;    This is for Connections Default is 3

    ;[LLC]                      ;    This Section is for IEEE 802.2
    ; RX.SIZE=2130              ;    Default is frame size is 2130

    ;[ODI]                      ;    This section is for ODI
    ; FRAME TOKEN-RING          ;    Frames for IPX/SPX  Frames
    ; FRAME TOKEN-RING_SNAP     ;    Frames for IP Frames
    ; ODI.NSUP=YES              ;    Use with Novells ODINSUP

    ;----------------------------END OF SMART.CFG ------------------------------;