# Installing Smart NDIS for LAN Manager

1. Run Madge Wizard to create a LAN Manager Madge driver installation disk.

2. Run the LAN Manager SETUP program.

3. Select Other Drivers, from the Network Adapter Drivers box. When prompted, insert the LAN Manager Madge driver installation disk created in 1, and press Enter.

4. Select All Madge Smart 16/4 Ringnodes (Smart NDIS).

5. Select the protocols you require, and continue through the SETUP process.

6. Save the configuration and exit from SETUP.

7. Reboot your computer.