# Smart 16/4 ISA Client PnP Ringnode

A high performance Plug 'n' Play Token Ring Adapter, optimised for client applications in today's fast ISA-bus PCs

| Overview Description Specifications Ordering Information

## Overview

The Smart 16/4 ISA Client PnP Ringnode is designed for use in ISA-based PCs, where the flexibility of Madge's memory-optimized Smart software is required.

Fully software configurable, the adapter provides the easiest, quickest adapter installation available. When used alongside other Plug 'n' Play devices, such as PnP-enabled sound cards, it works co-operatively with the other parts of the Plug 'n' Play system to automatically allocate system resources.

### Customer Benefits

- Simple and fast Plug 'n' Play installation
- Low overhead support of DOS desktops
- Optimized for 486 and Pentium-based PCs

### Key Features

- Certified for use with new 32-bit desktops
- Full support of Madge Smart software
- Excellent flexibility and performance
- Exceptional performance in today's complex LAN environments

## Description

- Introduction
- Easier, faster installation
- Investment protection for existing PCs and operating systems
- Powerful LAN support software
- Customer support without limits

### Introduction

The Smart 16/4 ISA Client PnP Ringnode is a fully Plug 'n' Play compliant Token Ring adapter, designed for use in today's high performance ISA-bus PCs. Ideal for running client applications, it can also be used in existing non-Plug 'n' Play PC environments. When used with a Plug 'n' Play PC and operating system (such as Windows 95), connecting to a network is easy: simply plug the adapter into the PC and power-on!

The Plug 'n' Play specification details hardware and software interfaces that allow a PC's BIOS and operating system to automatically configure adapter cards and other PC resources to avoid conflicts. In addition, Plug 'n' Play operating systems such as Microsoft's Windows 95 automatically load the protocol drivers and redirectors necessary to attach to file servers and other LAN resources.

As with all Madge Token Ring network products, the Smart 16/4 ISA Client PnP Ringnode is fully compliant with the IEEE 802.5 Token Ring standard. It can be freely mixed with IBM adapters and any other Token Ring adapters

### Easier, faster installation

The Plug 'n' Play specifications apply to PCs, adapter cards and operating systems. When all three elements are used together, configuration of the PC and adapters becomes completely automatic, eliminating the need for technical expertise to set up an operational PC system. Installation is faster and compatibility is assured. In addition, Madge's Smart WireSense circuitry automatically detects and drives the cable type used with the Smart 16/4 ISA Client PnP Ringnode.

When one or more elements of the system are not Plug 'n' Play, the extent of automation is reduced and user intervention in the installation process is likely to be required. However, installation benefits still accrue from those elements which are Plug 'n' Play.

### Investment protection for existing PCs and operating systems

The Smart 16/4 ISA Client PnP Ringnode is an ideal choice for non-Plug 'n' Play client PCs. Not only does it provide the major benefits and wide 3rd party compatibility of Madge's successful Smart 16/4 ISA Client Plus Ringnode, it also offers enhanced investment protection. When a future move is made to Plug 'n' Play PCs or operating systems, or when Plug 'n' Play support is added to the current choice of operating system, the Smart 16/4 ISA Client PnP Ringnode is ready to take advantage of this.

In non-Plug 'n' Play systems, easy-to-use software configuration makes the adapter quick and simple to install. Also included is a program for installing drivers and powerful diagnostics to verify correct operation of the Smart 16/4 ISA Client PnP Ringnode hardware. The utilities are intuitive and provide excellent context-sensitive help.

### Powerful LAN support software

The adapter is supplied with Madge's LAN Support Software; a complete set of drivers and utilities for all Smart 16/4 Ringnodes. This includes a range of host-resident Fastmac Plus drivers for highest performance, and Madge's unique adapter-resident Smart Software for multi-protocol flexibility.

With 128KB on-board memory, up to three protocols (from ODI, NDIS, LLC, NetBIOS, IPX or TCP/IP) can be downloaded concurrently, offering significant DOS memory savings over other driver configurations. Support is also offered for the latest Client-32 drivers which give further DOS memory configuration options.

### Customer support without limits

The Smart 16/4 ISA Client PnP Ringnode is backed by Madge's world-renowned expertise in networking. Madge's world-wide service and support organisation continues to satisfy the needs of our world-wide installed base of more than two million network adapters in the most demanding Global 1000 companies.

A world-wide network of field service engineers provide a wide range of technical services including on-site support and software upgrades. Customers can also download up-to-date technical information from on-line services such as CompuServe, or can contact the Madge World Wide Web Home page (http://www.madge.com). The Madge ISA Client PnP Ringnode adapter comes with a lifetime* hardware warranty and a 30-day installation guarantee, which includes free technical hot-line support and on-site assistance as required.

*Full details available on request

## Specifications

    Network type:               4 or 16 Mbps IBM and IEEE 802.5 Token Ring
    Supply voltage:             +5V DC
    Power:                      3W maximum
    Bus interface:              16-bit (8-bit ISA compatible);
                                Full Plug 'n' Play support
    Data transfer:              32-bit and 16-bit Programmed I/O
    Ring interface:	            9-pin D-type socket (STP);
                                RJ45 socket (UTP)
    EMI compatibility:          FCC Class A;
                                EN55022 (class B);
                                EN50082-1
    Memory:                     128 KB dynamic RAM on-board
    IRQ options:                2, 3, 5, 7, 10, 11, 15
    I/O options:                0920-093F, 0940-095F, 0960-097F, 0980-099F,
                                0A20-0A3F, 0A40-0A5F, 0A60-0A7F, 0A80-0A9F,
                                0B20-0B3F, 0B40-0B5F, 0B60-0B7F, 0B80-0B9F
    Boot ROM:                   Madge boot software
    Dimensions:                 157mm x 70mm
    Weight:                     0.11kg (approx)
    Temperature range:          0 - 50(C)
    Humidity range:             10% - 80% non-condensing
    Warranty period:            Lifetime*

## Ordering Information

    Part No    Description                           Qty  S/W & manuals

    22-04      Smart 16/4 ISA Client PnP Ringnode     1        1
    22-14      Smart 16/4 ISA Client PnP Ringnode    10        1
    22-24      Smart 16/4 ISA Client PnP Ringnode    20       20
    22-34      Smart 16/4 ISA Client PnP Ringnode    30        3
    22-54      Smart 16/4 ISA Client PnP Ringnode    50       50