# Firmware for other Smart 16/4 Ringnodes

The Smartroms that you can install onto the other Smart 16/4 Ringnodes are pre-programmed with one of two pieces of firmware:

- The Smartrom for remote booting using Remote Reset for NetWare has an image called NW.ROM loaded onto it.

- The Smartrom for remote booting using Remote Program Load for LAN Manager, LAN Server, Windows NT, or NetWare has an image called NRPL.ROM loaded onto it.

| Check that the part number on your Smartrom packaging includes the digits: 82-07 for NetWare Remote Reset. 82-08 for Remote Program Load. If it doesn't, contact your supplier.