# Running Artisoft LANtastic

This section describes the current level of support for the Artisoft LANtastic network operating system. Install the LANtastic workstation software by following the instructions in your LANtastic manual.

LANtastic uses a NetBIOS interface. To install a NetBIOS interface, use the SMART.EXE driver and the NETB.SMT protocol module. To do this, put the following line in CONFIG.SYS:
`device=SMART.EXE`
and create a SMART.CFG file with the following entries:
[HOST]
[CARD]
[NETB]

If you are also running any applications that require an LLC interface (for example, IBM AS400 support program), you need to add the [LLC] line to the SMART.CFG file.