# Installing the Smart NDIS driver

To install a Smart NDIS interface:

7 Select Network Card settings.

8 Select NDIS Token Ring. Type 5 as the interrupt setting. For the Bindings= option, type SMTNDIS_NIF.

9 Save the configuration.

10 Return to the main menu.

11 Ensure that the PROTOCOL.INI contains at least the following information:
`[PROTOCOL MANAGER]
DRIVERNAME = PROTMAN$
[VINES_XIF]
DRIVERNAME = NDISBAN$
BINDINGS = SMTNDIS_NIF
[SMTNDIS_NIF]
DRIVERNAME = SMART_NDIS$
Figure 1 Sample PROTOCOL.INI for VINES
` 12 Reboot the workstation. The Smart NDIS driver is now installed.

| To use Smart LLC interface (instead of Smart NDIS), install VINES and select 802.2 from the Network Card Settings menu in PCCONFIG. Load Smart LLC from CONFIG.SYS. To AUTOEXEC.BAT, add: ban /tokuiban