# NetWare for SAA (version 1.3 and 2.0)

The Madge driver MADGEODI.LAN supports NetWare for SAA.

To install the driver you require, perform the following steps in conjunction with the instructions in the NetWare for SAA manual:

1. Ensure that the following line appears in your AUTOEXEC.NCF file:
   LOAD < path> <driver> NAME = <boardname>
   where <path> is the location of the driver, <driver> is MADGEODI.LAN, and <boardname> is the identifier you are using for your adapter. (You may also need to set an LAA for the host connection.)

2. Install NetWare for SAA following the instructions in the NetWare for SAA manual.

3. Run CSCON. Select TOKEN RING when asked to specify the adapter.

4. When CSCON asks you to specify a Logical Adapter Name, type the <boardname> that you used in your AUTOEXEC.NCF file.