# Dedicated Token Ring (DTR)

In this directory you will find the Madge DTR drivers. These drivers are intended for use in server applications, and currently only support the Smart 16/4 EISA Ringnode and the Smart 16/4 PCI Ringnode (BM).

You will find an NDIS2 driver for use with IBM LanServer, an ODI driver for use with Netware servers and 32-bit NDIS driver for use in Windows NT servers.

NOTE: These drivers, apart from MADGEODI.LAN, have NOT been tested to the same level as the other drivers. They are pre-release versions of the drivers. You may substitute them for the LSS 5.0(2) drivers if you wish to evaluate DTR, but should be aware that they are not guaranteed to the same standards as the main LSS 5.0(2) drivers.

The Netware server driver, MADGEODI.LAN, has been updated and release tested in this release. This version of MADGEODI.LAN only supports DTR mode. Please use the driver in the \LSS.500\NETWARE\SERVER directory for Classic mode (non DTR) operation.

## Further Information

For further information please refer to the Readme file.