# Collage ATM Adapter

Ultimate ATM performance for data intensive applications

- Overview
- Description
- Specifications
- Ordering Information

## Overview

The Collage 155 Client/Server Adapter delivers the ultimate in performance at 155 Mbps to data-intensive server and high performance client applications. The adapter utilizes a high performance architecture and high-speed processor-based silicon technology for Segmentation and Reassembly (SAR). It offers multi-mode fiber or copper interfaces for flexible network integration. The easy-to-use management facility and local control and configuration capabilities ensure efficient, trouble-free operation.

### Customer Benefits

- Unsurpassed ATM performance at the desktop
- Investment protection with Madge LAN Emulation
- Fully ATM standards compliant

### Product Features

- Major software content
- High performance architecture
- Multi-mode fiber or copper interfaces

## Description

The Collage 155 Client/Server Adapter delivers the ultimate in performance at 155 Mbps to data-intensive server and high performance client applications.

- Introduction
- Madge ATM - the strategic choice
- Ultimate in performance
- Interoperability
- Industry leading LAN Emulation
- Efficient management and control
- Customer support without limits

### Introduction

Networking Technology represents a powerful tool in an increasingly competitive global business environment. Fast-emerging multimedia applications are also playing a critical role in worldwide communication. As these applications continue to develop, ATM is quickly becoming the only networking technology capable of effectively handling all types of networked information.

ATM breaks the bounds of today's internetworking technologies. It provides the dedicated, instantaneous bandwidth and quality of service essential for efficient transmission of voice, video and data. ATM matches the customer's need for high quality business communications.

### Madge ATM - the strategic choice

ATM is the only technology that can effectively integrate voice, video and data traffic at the desktop, to provide an affordable answer to today's business network needs. It is simply a better way to network needs. It is simply a better way to network and is rapidly being accepted as the network technology of choice. The Collage 155 PCI Adapter is part of a complete family of Madge products for workgroup ATM that includes workgroup switching as well as 25Mbps ATM adapters.

### Ultimate in performance

The Collage 155 PCI Adapter is a high performance, high efficiency ATM adapter that delivers the ultimate in performance for data intensive server and demanding client applications. These applications include distributed CAD/CAE and high resolution image retrieval such as those employed in the medical industry.

The adapter uses a high performance architecture and high-speed processor based silicon technology for Segmentation and Reassembly (SAR) together with well-tuned Madge Software to deliver unsurpassed ATM performance to the desktop.

Flexible traffic shaping (from 2kbps to 136Mbps) offers the ability to regulate transmission output to adhere to negotiated traffic speeds. Support for up to 1.024 virtual circuits will more than meet the needs of the most demanding new business applications.

### Interoperability

The Collage 155 PCI Adapter offers seamless interoperability with the Collage Family of ATM switches and adapters and integrates into all major client-server environments. Driver support includes NT, NetWare, DOS and Windows.

Through Madge's commitment to ATM Forum standards for LAN Emulation and SVC signaling, users also benefit from interoperability with a wide range of standards-based routers and switches.

### Industry leading LAN Emulation

Today's LAN applications are designed to run over a shared-media network such as Ethernet or Token Ring, ATM networks are connection-oriented. Madge's industry-leading LAN Emulation software, fully implementing the ATM Forum LAN software over ATM, and provides investment protection for today's legacy applications. Madge LAN Emulation software includes both Token Ring and Ethernet LEC, LECS, BUS and LES.

### Efficient management and control

The Collage 155 PCI Adapter offers an easy-to-use management facility that allows user access to configuration management and network performance monitoring. Complete statistics may be displayed on an individual virtual channel or adapter level basis. Local control and configuration capabilities ensure efficient, trouble-free operation.

### Customer support without limits

The Collage 155 PCI adapter is backed by Madge's world-renowned expertise in networking. Madge's worldwide service and support organization continues to satisfy the needs of our worldwide installed base of more than one million network adapters in the most demanding Global 1000 companies.

A worldwide network of field service engineers provide a wide range of technical services including on-site support and software upgrades. Customers can also download up-to-date technical information from on-line services such as CompuServe, or can contact the Madge World Wide Web home page (http://www.madge.com). The Collage 155 PCI adapter comes with a lifetime* hardware warranty and a 30-day installation guarantee, which includes free technical hot-line support and on-site assistance as required.

*Full details available on request

## Specifications

    Network Type:               Asynchronous Transfer Mode
    Access Speed:               155 Mbps
    ATM Standards:              UNI 3.0 (Q93B) & UNI 3.1
                                Q2931) Signaling and ILMI, AAL5 (SAR),
                                LAN Emulation (LANE) v1.0 LEC, LES,
                                LECS, BUS
    Virtual Circuit Capacity:   Transmit: 1,024 simultaneous VCs;
                                Receive: 1,024 simultaneous VCs
    Traffic Profiles:           1,024 separate profiles: 2kbps to 436
                                Mbps
    Flow Controls:              Software controlled (ABR Ready)
    Bus Interface:              32-bit PCI compatible
    Data Transfer:              Bus Mastered I/O
    Memory:                     28 KB SRAM
    Physical Interface:         UTP socket (RJ45) - Category 3 Cable or
                                above
                                Multi-mode fiber (SC connector)
    EMC Certification:          FCC Class A (Part 15, Subpart B);
                                EN 55022 Class A (UTP)
                                EN 55022 Class B (Fiber);
                                EN 50082-1
    Supply Voltage:             +5V DC+  5%
    Power:                      4 W maximum
    Dimensions:                 175mm x 107mm
    Weight:                     0.14kg (approx.)
    Temperature Range:          0-50 C
    Humidity Range:             10%-80% non-condensing
    Warranty:                   Lifetime*

    * Full details available upon request

    Specifications subject to change without notice

## Ordering Information

    Part No.  Description                              Qty  S/W & manuals
    32-01     Collage 155 PCI Adapter (fiber)           1      1
    32-11     Collage 155 PCI Adapter (fiber)-10 pack  10      1
    32-02     Collage 155 PCI Adapter (copper)          1      1
    32-12     Collage 155 PCI Adapter (copper)-10 pack 10      1