# Installing OS/2 Warp Connect with
LAN Requester v4.0

1. In the Product Selection dialog box, specify the products you need. If you want Internet access, check the IBM TCP/IP for OS/2 3.0 (includes Internet access) box.
2. Select Madge Smart Ringnodes for OS/2 v2.x.
3. Click Settings.
4. Click the LAN Requester tab in the top right-hand corner of the screen.
5. Type a Requester name and a Domain Name.
6. If you selected IBM TCP/IP earlier, type an IP address, subnet mask, and router address; then go to page 2 of the Setup Selected Products notepad, and type a TCP/IP Domain Name, and a Name Server.
7. Click Install.
8. After some minutes the Installation Completed dialog appears. Click OK.
9. The PC reboots.
10. Double-click on the MPTS icon on the OS/2 desktop.
11. Click OK.
12. Click Install.
13. Insert the Madge CSS Release Disk.
14. Type A:\OS2.
15. Click OK.
16. Click OK again.
17. Click Exit.
18. Click Exit again.
19. Click OK.
20. Click Exit.
21. Shutdown and reboot the PC.