# Inserting the Ringnode

To insert the Ringnode into your computer:

1. Remove the cover of your computer and select an empty Micro-Channel expansion slot.

2. Remove the slot's backplate. Keep its screw safely.

3. Push the Ringnode firmly into the slot. Do not force it. If it does not slide in easily, it may be misaligned.

4. Secure the Ringnode with the retaining screw.

5. Replace the cover of the computer.