# Supporting IBM TCP/IP or Wollongong Pathway Access for DOS workstations

IBM TCP/IP or Wollongong: ASI

1. Install IBM TCP/IP using the IBM Install program, or follow the instructions in the Wollongong manual for installing an IBM Token-Ring adapter.

2. Install the Smart LLC interface. For information about installing the Smart Software interfaces, see Installing the Smart Software for DOS workstations .

3. For IBM TCP/IP, edit your CONFIG.SYS file by replacing:
   IBMTR.DRV
   with:
   PCLAN.DRV /x:<irq number>/T

   Figure 1 shows a sample configuration for Wollongong.

    CONFIG.SYS:
    	DEVICE=PWTCP.SYS
    	DEVICE=SMART.EXE
    	REM LLC specified in SMART.CFG

    	AUTOEXEC.BAT:
    	TOKENRNG
    	PWTCP

Figure 1 Sample Wollongong configuration

IBM TCP/IP or Wollongong: ODI

Install the Smart ODI interface following the instructions in Installing the Smart Software for DOS workstations. For all combinations of ODI and TCP/IP specify the FRAME=Token_ring_SNAP parameter in your SMART.CFG file.