# Banyan Vines:
installing the NDIS2 driver onto a (DOS) workstation

The NDIS2 driver for DOS is called MCBND.DOS. To install it, perform the following in conjunction with the documentation supplied with Banyan Vines:

1. Copy the Vines LAN Software (DOS) Install disk to a directory on your workstation called C:\Vines. In this directory, run PCCONFIG.

2. From the main menu, select Network Card settings.

3. Select NDIS Token Ring. Type the adapter's interrupt setting. For the Bindings= option, type: MCBND_NIF.

4. Save the configuration and return to the main menu.

5. Copy all the files in the NDIS directory on the Vines (DOS) Workstation disks to C:\Vines on your workstation.

6. Copy MCBND.DOS from the Madge CSS Release Disk to C:\VINES.

7. Add the following lines to CONFIG.SYS:

   DEVICE=C:\Vines\PROTMAN.DOS /I: C:\Vines
   DEVICE=C:\Vines\MCBND.DOS

8. Add the following line to AUTOEXEC.BAT:

   BAN /NDTOKBAN

9. Ensure that the PROTOCOL.INI contains at least the information below.

       [PROTOCOL MANAGER]
        DRIVERNAME = PROTMAN$
             [VINES_XIF]
       	DRIVERNAME = NDISBAN$
       	BINDINGS = MCBND_NIF
         [MCBND_NIF]
       	DRIVERNAME = MCBND$

   Sample PROTOCOL.INI for Vines

10. Reboot the computer.