# Advanced configuration of Madge Ringnodes using Windows 95

To set advanced configuration options for Madge Smart Ringnodes:

1. Choose the Networks option from the Control panel. The screen displays the Network dialogue box.

2. Highlight the Madge Smart adapter in the components list.

3. Click on Properties. The screen displays the Properties dialogue box.

4. Click on the Advanced tab. You will see a list of options that you can set. For more information about these, proceed to Advanced configuration options.

5. Once you have finished setting the options, click on OK. The screen displays the Network dialog box.

6. Click on OK.