# Sample MADGECS.CFG file

    ; Configuration file for use with MADGECS

    EMULATE_SOCKET_SERVICES=YES    ; This line causes MADGECS to emulate socket services.

    EXCLUDE_IO=A20-AFF,            ; These lines delete particular I/O ranges from the
               1A20-1AFF,          ; list of available I/O ranges that MADGECS keeps.
               2A20-2AFF,
               3A20-3AFF,
               E20-EFF;

    DEFAULT_IO=NO                  ; This line forces MADGECS to use only the I/O ranges
                                   ; that you specify in MADGECS.CFG (see the USE_IO=
                                   ; option).

    USE_IO=300-31F, 4000-40FF      ; This line adds two ranges to MADGECS's list of
                                   ; available I/O ranges. The range 300-31F is of a size
                                   ; that is suitable for the PCMCIA Ringnode. The range
                                   ; 4000..40FF is of a size that is suitable for CardBus
                                   ; or PCMCIA adapters.

    DEFAULT_INTERRUPTS=NO          ; This line causes MADGECS to allocate only the
                                   ; interrupts that you specify in MADGECS.CFG (see
                                   ; the USE_INT= option).

    USE_INT=10,11                  ; This line causes MADGECS to add interrupts
                                   ; 10 and 11 to its list of available interrupts.

    DEFAULT_MEMORY=NO              ; This line forces MADGECS to use only the memory
                                   ; ranges that you specify in MADGECS.CFG (see the
                                   ; USE_MEMORY= option).

    USE_MEMORY=D000-DIFF           ; This line adds a memory range to MADGECS's
                                   ; list of available memory.