# Supporting Novell LAN WorkGroup for DOS

### Novell LAN WorkGroup for DOS version 5.0

### Novell LAN WorkGroup for DOS version 4.2

The instructions in this section apply to LAN WorkGroup for DOS version 4.2. They use the Madge Wizard program. The Madge Wizard program loads and configures the Madge drivers appropriate to your installation.

To load and configure Madge drivers:

1. Run the LAN WorkGroup for DOS INSTALL program. Select the None of these option from the list of adapter cards that is displayed during installation.

2. When you have installed LAN WorkGroup for DOS, insert Disk 1 of the Madge release disks into your A: drive. Run the Madge Wizard program by typing:
   `A:MWIZARD` [Enter]

3. Click on Set up Software.

4. Click on Maintain.

5. Select the drive and directory where you want the new files to be installed. Click on OK.
6. Highlight the Protocols needed option. Click on Edit.

7. Select TCP/IP (novell API). Click on Advanced. Enter the IP Configuration options. Click on OK.

8. Click on OK again. The screen displays the Manage current DOS boot setup screen.

9. Click on Install.