# Remote booting from Microsoft LAN Manager

This section tells you how to configure a LAN Manager version 2.2 or 2.1 server to perform Remote Program Load for DOS and OS/2 workstations. Read it in conjunction with the instructions about installing Remote Program Load on a server, in the LAN Manager Administrator’s Guide.

Before you install your driver software:

- Configure the Smartrom to use Remote Program Load. For information about this, see Configuring your Smartrom.

- Follow the instructions in the LAN Manager Administrator’s Guide for remote booting with IBM Token-Ring adapters. Then follow the instructions in this chapter.

| Workstations that use the Remote Program Load booting scheme automatically remote boot across source-routing bridges.

Remote booting DOS workstations from LAN Manager

Remote booting OS/2 workstations from LAN Manager