# Configuration information for the AT Plus Ringnode, PCI Ringnode, or ISA Client Plus Ringnode

| For the AT Plus, a switch is ON when it is down. If you alter any switch settings, run the configuration software to re-enable the Ringnode.

Contents

Computers with a floppy drive

Diskless workstations

AT mode

Computers with a floppy drive

Run Madge Wizard to configure the AT Plus, PCI and ISA Client Plus Ringnodes.

Diskless workstations

To configure the AT Plus Ringnode in a diskless workstation, first enable the Smartrom by setting switch 3 to ON. Then reboot. Run the configuration software from the Smartrom by pressing [F1] at the prompt.

You cannot configure the ISA Client Plus in a diskless workstation until you have enabled the Smartrom. To do this, install the Ringnode into a computer with a hard or floppy drive. Run the configuration software and choose the option that enables the Smartrom. Then remove the Ringnode and install it into the diskless workstation. To configure the Ringnode further, reboot and press [F1] at the prompt.

AT mode

If you are operating an AT Plus Ringnode in AT mode, set switches 1, 2, 3, and 4. In AT mode these settings are not software configurable. After you have set the switches, however, you must run the configuration software. Until you do so, your Ringnode is disabled. (The Ringnode is supplied in Normal mode.)

Switch 1 | Switch 2 | I/O address | ROM address
OFF | OFF (Default) | 0A20-0A2F | CC000-CDFFF
ON | OFF | 1A20-1A2F | DC000-DDFFF
OFF | ON | 2A20-2A2F | CE000-CFFFF
ON | ON | 3A20-3A2F | DE000-DFFFF

Settings for AT Plus switches 1 and 2