# OS2: Card and Socket Services

To use the Madge 16/4 CardBus Adapter, you must use the Madge Card Services software by copying the file MADGECS.SYS from the Madge CSS Release Disk.

Run MADGECS.SYS from CONFIG.SYS. A sample device line is DEVICE=C:\MADGECS.SYS.

| Note that MADGECS.SYS does not emulate Socket Services. The Socket Services facility is only available with the DOS version of the utility (MADGECS.EXE).

| Note that the MADGECS software is only for the Madge CardBus and PCMCIA adapters; it does not work with PC Cards from other manufacturers. Therefore, when the CardBus version of PCMCIA.SYS becomes available from IBM, we recommend you to use that.

[Back to adapter installation instructions]