# The Miniport driver

The miniport (NDIS3) driver MDGMPORT.SYS supports the following environments:

Environments | Protocols they use
IBM LAN Server | NetBIOS
MS LAN Manager | NetBIOS
Windows NT Server | NetBIOS
3270 Applications | LLC

| Configuring the 32-bit Microsoft Data Link Control (DLC) interface over the Miniport driver, MDGMPORT.SYS.

You can use the Madge Smart 16/4 PCMCIA Ringnode with Windows 95 and Windows NT versions 3.51 and 4.0

You can make an unattended installation of Windows 95 or Windows NT 4.0 using the Miniport driver