# Smartrom for NetWare Remote Reset

### Error codes:

E9901 Error initializing Network Interface Board

If the above message is displayed, ensure that your cable is inserted correctly. Then reboot your workstation.

Opening boot-image on file server <SERVER NAME> Error finding server

If the above message is displayed, ensure that server <NAME> exists on the network, and is running.

(No error code) Opening boot-image file on server <SERVER NAME> Error opening boot-disk image file

If the above message is displayed, determine the name of the boot-image file that the Smartrom is looking for by running SMARTROM.EXE with the /LIST option (at the prompt, type: smartrom /list [Enter]). Then check that the file exists in the SYS\LOGIN directory of the server called <SERVER NAME>.