# Editing a hardware configuration script

|  | for more information about editing a hardware configuration script, see MWSCRIPT.TXT. (When you have finished reading the topic, click on the browser's back button to return to this screen).

Hardware scripts are saved as text files and may be modified using a text editor.

There are three examples of hardware configuration scripts which can be found on the LSS CD in the directory \LSS.500\MWIZARD\SCRIPTS:

- The EXAMPLE1.HWR script gives a full list of the available options. You can create your own script files by editing the file to remove the semi-colon from in front of the options you wish to enable.

- EXAMPLE2.HWR is a short script to enable a Smartrom.

- EXAMPLE3.HWR is a short script to change 4Mbps ring speed to 16Mbps.