# Microsoft LAN Manager:
installing the NDIS2 driver

The Madge NDIS2 driver for OS/2 is called MCBND.OS2. To install it, follow the instructions below:

1. Run the LAN Manager SETUP utility.
2. From the Network Adapter Drivers box, select Other Drivers.
3. When prompted, put the Madge CSS Release Disk into the floppy drive, and press [Enter].
4. Select Madge 16/4 CardBus Adapter.
5. Select the protocols you require.
6. Save your configuration.
7. Exit SETUP.
8. Shut down and reboot the computer. MCBND.OS2 is now installed.