# Configuring Hardware Wizard

To run Madge Wizard using command-line options, boot your computer, then at the DOS prompt type:

`MWIZARD HARDWARE <command-line options>`

The command-line options that you can use to configure Hardware Wizard (Change Ringnode configuration) are:

Use this command-line option: | If you want to:
SCRIPTING | Create a hardware install script.
LOAD=<script file name.HWR> | Load and run a hardware install script.
LOAD=<script file name.HWR> NOSCRIPTERRORS | Turn off all warnings and errors when a script is run.
NOINITWARNINGS | Turn off all initial warnings and errors during ringnode discovery.